@prefix fhir: <http://hl7.org/fhir/> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .

# - resource -------------------------------------------------------------------

[] a fhir:NamingSystem;
  fhir:Resource.id [ fhir:value "imei-identifier"];
  fhir:DomainResource.text [
     fhir:Narrative.status [ fhir:value "generated" ]
  ];
  fhir:DomainResource.extension [
     fhir:index 0;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.url" ];
     fhir:Extension.value [ fhir:value "http://terminology.hl7.org/NamingSystem/imei-identifier" ]
  ], [
     fhir:index 1;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.version" ];
     fhir:Extension.value [ fhir:value "1.0.0" ]
  ], [
     fhir:index 2;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.title" ];
     fhir:Extension.value [ fhir:value "IMEI as a device identifier" ]
  ];
  fhir:NamingSystem.name [ fhir:value "IMEI_Identifier"];
  fhir:NamingSystem.status [ fhir:value "active"];
  fhir:NamingSystem.kind [ fhir:value "identifier"];
  fhir:NamingSystem.date [ fhir:value "2021-06-14T00:00:00-00:00"];
  fhir:NamingSystem.publisher [ fhir:value "IHE Patient Care Devices (PCD)"];
  fhir:NamingSystem.contact [
     fhir:index 0;
     fhir:ContactDetail.name [ fhir:value "Devices on FHIR working group; IHE Patient Care Devices" ]
  ];
  fhir:NamingSystem.responsible [ fhir:value "IHE Patient Care Devices"];
  fhir:NamingSystem.description [ fhir:value "The International Mobile Equipment Identity (IMEI) is a number, usually unique, to identify 3GPP and iDEN mobile phones, as well as some satellite phones. The IMEI consists of 15 decimal digits: 14 digits plus a check digit while the IMEISV consists of 16 decimal digits: 14 digits plus two software version digits. These numbers includes information on the origin, model, and serial number of the device. The structure of the IMEI/SV is specified in 3GPP TS 23.003. The model and origin comprise the initial 8-digit portion of the IMEI/SV, known as the Type Allocation Code (TAC). The remainder of the IMEI is manufacturer-defined, with a Luhn check digit at the end."];
  fhir:NamingSystem.uniqueId [
     fhir:index 0;
     fhir:NamingSystem.type [ fhir:value "uri" ];
     fhir:NamingSystem.value [ fhir:value "http://hl7.org/fhir/sid/imei" ];
     fhir:NamingSystem.preferred [ fhir:value "true" ];
     fhir:NamingSystem.comment [ fhir:value "International Mobile Equipment Identity (IMEI) number" ]
  ] .

# -------------------------------------------------------------------------------------

