@prefix fhir: <http://hl7.org/fhir/> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .

# - resource -------------------------------------------------------------------

[] a fhir:NamingSystem;
  fhir:Resource.id [ fhir:value "zigbee-address-identifier"];
  fhir:DomainResource.text [
     fhir:Narrative.status [ fhir:value "generated" ]
  ];
  fhir:DomainResource.extension [
     fhir:index 0;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.url" ];
     fhir:Extension.value [ fhir:value "http://terminology.hl7.org/NamingSystem/zigbee-address-identifier" ]
  ], [
     fhir:index 1;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.version" ];
     fhir:Extension.value [ fhir:value "1.0.0" ]
  ], [
     fhir:index 2;
     fhir:Extension.url [ fhir:value "http://hl7.org/fhir/5.0/StructureDefinition/extension-NamingSystem.title" ];
     fhir:Extension.value [ fhir:value "ZigBee Address as a device identifier" ]
  ];
  fhir:NamingSystem.name [ fhir:value "ZigBee_Address_Identifier"];
  fhir:NamingSystem.status [ fhir:value "active"];
  fhir:NamingSystem.kind [ fhir:value "identifier"];
  fhir:NamingSystem.date [ fhir:value "2021-06-14T00:00:00-00:00"];
  fhir:NamingSystem.publisher [ fhir:value "IHE Patient Care Devices (PCD)"];
  fhir:NamingSystem.contact [
     fhir:index 0;
     fhir:ContactDetail.name [ fhir:value "Devices on FHIR working group; IHE Patient Care Devices" ]
  ];
  fhir:NamingSystem.responsible [ fhir:value "IHE Patient Care Devices"];
  fhir:NamingSystem.description [ fhir:value "The ZigBee Address is a unique 64-bit identifier assigned to each ZigBee device by the manufacturer. ZigBee Addresses are usually displayed as 8 bytes written in hexadecimal and separated by colons (example - DF:3B:00:11:22:33:FF:EE). They are an essential part of ZigBee-based protocols. The most-significant 24 bits of the ZigBee address is the so-called Organizationally Unique Identifier (OUI). It can be used to determine the manufacturer of a device. OUI prefixes are assigned by the Institute of Electrical and Electronics Engineers (IEEE). An EUI (Extended Unique Identifier) is generally made from an OUI and thus a ZigBee Address is also an EUI-64. When a ZigBee device joins a network it is assigned an additional 16-bit address sometimes referred to as its network address. This address is different from the 64-bit ZigBee address and is dynamic."];
  fhir:NamingSystem.uniqueId [
     fhir:index 0;
     fhir:NamingSystem.type [ fhir:value "uri" ];
     fhir:NamingSystem.value [ fhir:value "http://hl7.org/fhir/sid/eui-64/zigbee" ];
     fhir:NamingSystem.preferred [ fhir:value "true" ];
     fhir:NamingSystem.comment [ fhir:value "ZigBee address" ]
  ] .

# -------------------------------------------------------------------------------------

