@prefix fhir: <http://hl7.org/fhir/> .
@prefix owl: <http://www.w3.org/2002/07/owl#> .
@prefix rdf: <http://www.w3.org/1999/02/22-rdf-syntax-ns#> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
@prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

# - resource -------------------------------------------------------------------

<http://terminology.hl7.org/NamingSystem/imei-identifier> a fhir:NamingSystem ;
  fhir:nodeRole fhir:treeRoot ;
  fhir:id [ fhir:v "imei-identifier"] ; # 
  fhir:text [
     fhir:status [ fhir:v "generated" ] ;
     fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: NamingSystem imei-identifier</b></p><a name=\"imei-identifier\"> </a><a name=\"hcimei-identifier\"> </a><a name=\"imei-identifier-en-US\"> </a><h3>Summary</h3><table class=\"grid\"><tr><td>Defining URL</td><td>http://terminology.hl7.org/NamingSystem/imei-identifier</td></tr><tr><td>Version</td><td>1.0.0</td></tr><tr><td>Name</td><td>IMEI_Identifier</td></tr><tr><td>Title</td><td>IMEI as a device identifier</td></tr><tr><td>Status</td><td>active</td></tr><tr><td>Definition</td><td><div><p>The International Mobile Equipment Identity (IMEI) is a number, usually unique, to identify 3GPP and iDEN mobile phones, as well as some satellite phones. The IMEI consists of 15 decimal digits: 14 digits plus a check digit while the IMEISV consists of 16 decimal digits: 14 digits plus two software version digits. These numbers includes information on the origin, model, and serial number of the device. The structure of the IMEI/SV is specified in 3GPP TS 23.003. The model and origin comprise the initial 8-digit portion of the IMEI/SV, known as the Type Allocation Code (TAC). The remainder of the IMEI is manufacturer-defined, with a Luhn check digit at the end.</p>\n</div></td></tr><tr><td>Publisher</td><td>IHE Patient Care Devices (PCD)</td></tr></table><h3>Identifiers</h3><table class=\"grid\"><tr><td><b>Type</b></td><td><b>Value</b></td><td><b>Preferred</b></td><td><b>Comment</b></td></tr><tr><td>URI</td><td>http://hl7.org/fhir/sid/imei</td><td>true</td><td>International Mobile Equipment Identity (IMEI) number</td></tr></table></div>"^^rdf:XMLLiteral
  ] ; # 
  fhir:url [ fhir:v "http://terminology.hl7.org/NamingSystem/imei-identifier"^^xsd:anyURI] ; # 
  fhir:version [ fhir:v "1.0.0"] ; # 
  fhir:name [ fhir:v "IMEI_Identifier"] ; # 
  fhir:title [ fhir:v "IMEI as a device identifier"] ; # 
  fhir:status [ fhir:v "active"] ; # 
  fhir:kind [ fhir:v "identifier"] ; # 
  fhir:date [ fhir:v "2021-06-14T00:00:00-00:00"^^xsd:dateTime] ; # 
  fhir:publisher [ fhir:v "IHE Patient Care Devices (PCD)"] ; # 
  fhir:contact ( [
     fhir:name [ fhir:v "Devices on FHIR working group; IHE Patient Care Devices" ]
  ] ) ; # 
  fhir:responsible [ fhir:v "IHE Patient Care Devices"] ; # 
  fhir:description [ fhir:v "The International Mobile Equipment Identity (IMEI) is a number, usually unique, to identify 3GPP and iDEN mobile phones, as well as some satellite phones. The IMEI consists of 15 decimal digits: 14 digits plus a check digit while the IMEISV consists of 16 decimal digits: 14 digits plus two software version digits. These numbers includes information on the origin, model, and serial number of the device. The structure of the IMEI/SV is specified in 3GPP TS 23.003. The model and origin comprise the initial 8-digit portion of the IMEI/SV, known as the Type Allocation Code (TAC). The remainder of the IMEI is manufacturer-defined, with a Luhn check digit at the end."] ; # 
  fhir:uniqueId ( [
     fhir:type [ fhir:v "uri" ] ;
     fhir:value [ fhir:v "http://hl7.org/fhir/sid/imei" ] ;
     fhir:preferred [ fhir:v "true"^^xsd:boolean ] ;
     fhir:comment [ fhir:v "International Mobile Equipment Identity (IMEI) number" ]
  ] ) . # 

# -------------------------------------------------------------------------------------

