@prefix fhir: <http://hl7.org/fhir/> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .

# - resource -------------------------------------------------------------------

[] a fhir:NamingSystem ;
  fhir:id [ fhir:v "imei-identifier"] ;
  fhir:text [
     fhir:status [ fhir:v "generated" ]
  ] ;
  fhir:url [ fhir:v "http://terminology.hl7.org/NamingSystem/imei-identifier"], [ fhir:v "http://terminology.hl7.org/NamingSystem/imei-identifier"] ;
  fhir:version [ fhir:v "1.0.0"], [ fhir:v "1.0.0"] ;
  fhir:name [ fhir:v "IMEI_Identifier"], [ fhir:v "IMEI_Identifier"] ;
  fhir:title [ fhir:v "IMEI as a device identifier"], [ fhir:v "IMEI as a device identifier"] ;
  fhir:status [ fhir:v "active"], [ fhir:v "active"] ;
  fhir:date [ fhir:v "2021-06-14T00:00:00-00:00"], [ fhir:v "2021-06-14T00:00:00-00:00"] ;
  fhir:publisher [ fhir:v "IHE Patient Care Devices (PCD)"], [ fhir:v "IHE Patient Care Devices (PCD)"] ;
  fhir:contact ( [
     fhir:name [ fhir:v "Devices on FHIR working group; IHE Patient Care Devices" ]
  ] [
     fhir:name [ fhir:v "Devices on FHIR working group; IHE Patient Care Devices" ]
  ] ) ;
  fhir:description [ fhir:v "The International Mobile Equipment Identity (IMEI) is a number, usually unique, to identify 3GPP and iDEN mobile phones, as well as some satellite phones. The IMEI consists of 15 decimal digits: 14 digits plus a check digit while the IMEISV consists of 16 decimal digits: 14 digits plus two software version digits. These numbers includes information on the origin, model, and serial number of the device. The structure of the IMEI/SV is specified in 3GPP TS 23.003. The model and origin comprise the initial 8-digit portion of the IMEI/SV, known as the Type Allocation Code (TAC). The remainder of the IMEI is manufacturer-defined, with a Luhn check digit at the end."], [ fhir:v "The International Mobile Equipment Identity (IMEI) is a number, usually unique, to identify 3GPP and iDEN mobile phones, as well as some satellite phones. The IMEI consists of 15 decimal digits: 14 digits plus a check digit while the IMEISV consists of 16 decimal digits: 14 digits plus two software version digits. These numbers includes information on the origin, model, and serial number of the device. The structure of the IMEI/SV is specified in 3GPP TS 23.003. The model and origin comprise the initial 8-digit portion of the IMEI/SV, known as the Type Allocation Code (TAC). The remainder of the IMEI is manufacturer-defined, with a Luhn check digit at the end."] ;
  fhir:kind [ fhir:v "identifier"] ;
  fhir:responsible [ fhir:v "IHE Patient Care Devices"] ;
  fhir:uniqueId ( [
     fhir:type [ fhir:v "uri" ] ;
     fhir:value [ fhir:v "http://hl7.org/fhir/sid/imei" ] ;
     fhir:preferred [ fhir:v "true" ] ;
     fhir:comment [ fhir:v "International Mobile Equipment Identity (IMEI) number" ]
  ] ) .

# -------------------------------------------------------------------------------------

