@prefix fhir: <http://hl7.org/fhir/> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .

# - resource -------------------------------------------------------------------

[] a fhir:NamingSystem ;
  fhir:id [ fhir:v "zigbee-address-identifier"] ;
  fhir:text [
     fhir:status [ fhir:v "generated" ]
  ] ;
  fhir:url [ fhir:v "http://terminology.hl7.org/NamingSystem/zigbee-address-identifier"], [ fhir:v "http://terminology.hl7.org/NamingSystem/zigbee-address-identifier"] ;
  fhir:version [ fhir:v "1.0.0"], [ fhir:v "1.0.0"] ;
  fhir:name [ fhir:v "ZigBee_Address_Identifier"], [ fhir:v "ZigBee_Address_Identifier"] ;
  fhir:title [ fhir:v "ZigBee Address as a device identifier"], [ fhir:v "ZigBee Address as a device identifier"] ;
  fhir:status [ fhir:v "active"], [ fhir:v "active"] ;
  fhir:date [ fhir:v "2021-06-14T00:00:00-00:00"], [ fhir:v "2021-06-14T00:00:00-00:00"] ;
  fhir:publisher [ fhir:v "IHE Patient Care Devices (PCD)"], [ fhir:v "IHE Patient Care Devices (PCD)"] ;
  fhir:contact ( [
     fhir:name [ fhir:v "Devices on FHIR working group; IHE Patient Care Devices" ]
  ] [
     fhir:name [ fhir:v "Devices on FHIR working group; IHE Patient Care Devices" ]
  ] ) ;
  fhir:description [ fhir:v "The ZigBee Address is a unique 64-bit identifier assigned to each ZigBee device by the manufacturer. ZigBee Addresses are usually displayed as 8 bytes written in hexadecimal and separated by colons (example - DF:3B:00:11:22:33:FF:EE). They are an essential part of ZigBee-based protocols. The most-significant 24 bits of the ZigBee address is the so-called Organizationally Unique Identifier (OUI). It can be used to determine the manufacturer of a device. OUI prefixes are assigned by the Institute of Electrical and Electronics Engineers (IEEE). An EUI (Extended Unique Identifier) is generally made from an OUI and thus a ZigBee Address is also an EUI-64. When a ZigBee device joins a network it is assigned an additional 16-bit address sometimes referred to as its network address. This address is different from the 64-bit ZigBee address and is dynamic."], [ fhir:v "The ZigBee Address is a unique 64-bit identifier assigned to each ZigBee device by the manufacturer. ZigBee Addresses are usually displayed as 8 bytes written in hexadecimal and separated by colons (example - DF:3B:00:11:22:33:FF:EE). They are an essential part of ZigBee-based protocols. The most-significant 24 bits of the ZigBee address is the so-called Organizationally Unique Identifier (OUI). It can be used to determine the manufacturer of a device. OUI prefixes are assigned by the Institute of Electrical and Electronics Engineers (IEEE). An EUI (Extended Unique Identifier) is generally made from an OUI and thus a ZigBee Address is also an EUI-64. When a ZigBee device joins a network it is assigned an additional 16-bit address sometimes referred to as its network address. This address is different from the 64-bit ZigBee address and is dynamic."] ;
  fhir:kind [ fhir:v "identifier"] ;
  fhir:responsible [ fhir:v "IHE Patient Care Devices"] ;
  fhir:uniqueId ( [
     fhir:type [ fhir:v "uri" ] ;
     fhir:value [ fhir:v "http://hl7.org/fhir/sid/eui-64/zigbee" ] ;
     fhir:preferred [ fhir:v "true" ] ;
     fhir:comment [ fhir:v "ZigBee address" ]
  ] ) .

# -------------------------------------------------------------------------------------

